CMC translator:

hu - Hui ID switcher

Global:
oo =Windows=1/mac=2 ID
gc - selected HUI channel
gj - send id (A-E)
gp - gc+16 (+10 hex) for receive pan number
gr - read toggle value (gets a reset with cursor up/down)
gw - write toggle value (gets a reset with cursor up/down)
ha - selected channel on/off
he - selected channel off temp. status for switching CH on/off
hf - selected channel on temp. status for switching CH on/off
hi - no selected channel status
ho - rude solo state reset
hp - insert/param status

FD: 
ga - FD shift on/off
hm - faders show meters
h0 - bank by 4 channels on/off

CH to HUI: 
gc - selected HUI channel
gd - selected HUI channel edited +32 (+20 hex) for second fader value
gf - flip mode on/off
gj - send id (A-E)
gk - pan send status
gp - gc+16 (+10 hex) for receive pan number 
gq - switch panner/send mode (gedeeld met QC)
gr - read toggle value (wordt gereset bij cursor up/down)
gs - CH shift on/off
gw - write toggle value (wordt gereset bij cursor up/down)
gx - write/read status (reset bij cursor up/down)
hb - bank on hold status
ho - rude solo state

CH from HUI:
gc - selected HUI channel
gj - send id (A-E)
gk - pan send status
gq - switch panner/send mode (gedeeld met QC)
ho - solo is aan (op willekeurige track) 
hy - fader jump/catch mode

TP to HUI:
gb - toggle slip/grid 
gg - previous slider value
gh - current slider value
hg - previous filtered slider value
hh - current filtered slider value
hj - jog mode/state scrub/shuttle
gn - locate mode (click <</>> en pref./next boundary)
go - slider mode button on/off
gt - slider mode (0-5)
gu - TP shift on/off
gz - Touch slider on/off

TP from HUI:
gt - slider mode (0-5)
hz - zoom mode on/off

AI to HUI:
gl - toggle JOG step-/region mode
gm - AI unit mode
hc - AI knob click on/off
hd - toggles scroll direction

AI from HUI:
hm = mixer status

QC to HUI:
gf - flip mode on/off
gi - scroll knob value
gj - send id (A-E)
gk - pan send status
gq - QC unit mode
gr - read toggle value (wordt gereset bij cursor up/down)
gx - write/read status
gv - QC shift on/off
gw - write toggle value (wordt gereset bij cursor up/down)
hb - bank on hold status
hs - f/Q as shift button 
ht - block transport functions (when setting send id)
hu - plug-in window open/close status
hw - write on any channel status
hx - allow switch plug-in on off / plug-in window on/off

ia=volume fader value selected track

QC from HUI:
gy - QC knob value +0 or +16 (send/pan receive)